    001    package org.apache.commons.net.ntp;
    002    /*
    003     * Licensed to the Apache Software Foundation (ASF) under one or more
    004     * contributor license agreements.  See the NOTICE file distributed with
    005     * this work for additional information regarding copyright ownership.
    006     * The ASF licenses this file to You under the Apache License, Version 2.0
    007     * (the "License"); you may not use this file except in compliance with
    008     * the License.  You may obtain a copy of the License at
    009     *
    010     *      http://www.apache.org/licenses/LICENSE-2.0
    011     *
    012     * Unless required by applicable law or agreed to in writing, software
    013     * distributed under the License is distributed on an "AS IS" BASIS,
    014     * WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied.
    015     * See the License for the specific language governing permissions and
    016     * limitations under the License.
    017     */
    018
    019
    020    import java.util.ArrayList;
    021    import java.util.List;
    022
    023    /**
    024     * Wrapper class to network time packet messages (NTP, etc) that computes
    025     * related timing info and stats.
    026     *
    027     * @author Jason Mathews, MITRE Corp
    028     *
    029     * @version $Revision: 1299238 $
    030     */
    031    public class TimeInfo {
    032
    033        private final NtpV3Packet _message;
    034        private List<String> _comments;
    035        private Long _delay;
    036        private Long _offset;
    037
    038        /**
    039         * time at which time message packet was received by local machine
    040         */
    041        private final long _returnTime;
    042
    043        /**
    044         * flag indicating that the TimeInfo details was processed and delay/offset were computed
    045         */
    046        private boolean _detailsComputed;
    047
    048        /**
    049         * Create TimeInfo object with raw packet message and destination time received.
    050         *
    051         * @param message NTP message packet
    052         * @param returnTime  destination receive time
    053         * @throws IllegalArgumentException if message is null
    054         */
    055        public TimeInfo(NtpV3Packet message, long returnTime) {
    056            this(message, returnTime, null, true);
    057        }
    058
    059        /**
    060         * Create TimeInfo object with raw packet message and destination time received.
    061         *
    062         * @param message NTP message packet
    063         * @param returnTime  destination receive time
    064         * @param comments List of errors/warnings identified during processing
    065         * @throws IllegalArgumentException if message is null
    066         */
    067        public TimeInfo(NtpV3Packet message, long returnTime, List<String> comments)
    068        {
    069                this(message, returnTime, comments, true);
    070        }
    071
    072        /**
    073         * Create TimeInfo object with raw packet message and destination time received.
    074         * Auto-computes details if computeDetails flag set otherwise this is delayed
    075         * until computeDetails() is called. Delayed computation is for fast
    076         * intialization when sub-millisecond timing is needed.
    077         *
    078         * @param msgPacket NTP message packet
    079         * @param returnTime  destination receive time
    080         * @param doComputeDetails  flag to pre-compute delay/offset values
    081         * @throws IllegalArgumentException if message is null
    082         */
    083        public TimeInfo(NtpV3Packet msgPacket, long returnTime, boolean doComputeDetails)
    084        {
    085                this(msgPacket, returnTime, null, doComputeDetails);
    086        }
    087
    088        /**
    089         * Create TimeInfo object with raw packet message and destination time received.
    090         * Auto-computes details if computeDetails flag set otherwise this is delayed
    091         * until computeDetails() is called. Delayed computation is for fast
    092         * intialization when sub-millisecond timing is needed.
    093         *
    094         * @param message NTP message packet
    095         * @param returnTime  destination receive time
    096         * @param comments  list of comments used to store errors/warnings with message
    097         * @param doComputeDetails  flag to pre-compute delay/offset values
    098         * @throws IllegalArgumentException if message is null
    099         */
    100        public TimeInfo(NtpV3Packet message, long returnTime, List<String> comments,
    101                       boolean doComputeDetails)
    102        {
    103            if (message == null) {
    104                throw new IllegalArgumentException("message cannot be null");
    105            }
    106            this._returnTime = returnTime;
    107            this._message = message;
    108            this._comments = comments;
    109            if (doComputeDetails) {
    110                computeDetails();
    111            }
    112        }
    113
    114        /**
    115         * Add comment (error/warning) to list of comments associated
    116         * with processing of NTP parameters. If comment list not create
    117         * then one will be created.
    118         *
    119         * @param comment
    120         */
    121        public void addComment(String comment)
    122        {
    123            if (_comments == null) {
    124                _comments = new ArrayList<String>();
    125            }
    126            _comments.add(comment);
    127        }
    128
    129        /**
    130         * Compute and validate details of the NTP message packet. Computed
    131         * fields include the offset and delay.
    132         */
    133        public void computeDetails()
    134        {
    135            if (_detailsComputed) {
    136                return; // details already computed - do nothing
    137            }
    138            _detailsComputed = true;
    139            if (_comments == null) {
    140                _comments = new ArrayList<String>();
    141            }
    142
    143            TimeStamp origNtpTime = _message.getOriginateTimeStamp();
    144            long origTime = origNtpTime.getTime();
    145
    146            // Receive Time is time request received by server (t2)
    147            TimeStamp rcvNtpTime = _message.getReceiveTimeStamp();
    148            long rcvTime = rcvNtpTime.getTime();
    149
    150            // Transmit time is time reply sent by server (t3)
    151            TimeStamp xmitNtpTime = _message.getTransmitTimeStamp();
    152            long xmitTime = xmitNtpTime.getTime();
    153
    154            /*
    155             * Round-trip network delay and local clock offset (or time drift) is calculated
    156             * according to this standard NTP equation:
    157             *
    158             * LocalClockOffset = ((ReceiveTimestamp - OriginateTimestamp) +
    159             *                     (TransmitTimestamp - DestinationTimestamp)) / 2
    160             *
    161             * equations from RFC-1305 (NTPv3)
    162             *      roundtrip delay = (t4 - t1) - (t3 - t2)
    163             *      local clock offset = ((t2 - t1) + (t3 - t4)) / 2
    164             *
    165             * It takes into account network delays and assumes that they are symmetrical.
    166             *
    167             * Note the typo in SNTP RFCs 1769/2030 which state that the delay
    168             * is (T4 - T1) - (T2 - T3) with the "T2" and "T3" switched.
    169             */
    170            if (origNtpTime.ntpValue() == 0)
    171            {
    172                // without originate time cannot determine when packet went out
    173                // might be via a broadcast NTP packet...
    174                if (xmitNtpTime.ntpValue() != 0)
    175                {
    176                    _offset = Long.valueOf(xmitTime - _returnTime);
    177                    _comments.add("Error: zero orig time -- cannot compute delay");
    178                } else {
    179                    _comments.add("Error: zero orig time -- cannot compute delay/offset");
    180                }
    181            } else if (rcvNtpTime.ntpValue() == 0 || xmitNtpTime.ntpValue() == 0) {
    182                _comments.add("Warning: zero rcvNtpTime or xmitNtpTime");
    183                // assert destTime >= origTime since network delay cannot be negative
    184                if (origTime > _returnTime) {
    185                    _comments.add("Error: OrigTime > DestRcvTime");
    186                } else {
    187                    // without receive or xmit time cannot figure out processing time
    188                    // so delay is simply the network travel time
    189                    _delay = Long.valueOf(_returnTime - origTime);
    190                }
    191                // TODO: is offset still valid if rcvNtpTime=0 || xmitNtpTime=0 ???
    192                // Could always hash origNtpTime (sendTime) but if host doesn't set it
    193                // then it's an malformed ntp host anyway and we don't care?
    194                // If server is in broadcast mode then we never send out a query in first place...
    195                if (rcvNtpTime.ntpValue() != 0)
    196                {
    197                    // xmitTime is 0 just use rcv time
    198                    _offset = Long.valueOf(rcvTime - origTime);
    199                } else if (xmitNtpTime.ntpValue() != 0)
    200                {
    201                    // rcvTime is 0 just use xmitTime time
    202                    _offset = Long.valueOf(xmitTime - _returnTime);
    203                }
    204            } else
    205            {
    206                 long delayValue = _returnTime - origTime;
    207                 // assert xmitTime >= rcvTime: difference typically < 1ms
    208                 if (xmitTime < rcvTime)
    209                 {
    210                     // server cannot send out a packet before receiving it...
    211                     _comments.add("Error: xmitTime < rcvTime"); // time-travel not allowed
    212                 } else
    213                 {
    214                     // subtract processing time from round-trip network delay
    215                     long delta = xmitTime - rcvTime;
    216                     // in normal cases the processing delta is less than
    217                     // the total roundtrip network travel time.
    218                     if (delta <= delayValue)
    219                     {
    220                         delayValue -= delta; // delay = (t4 - t1) - (t3 - t2)
    221                     } else
    222                     {
    223                         // if delta - delayValue == 1 ms then it's a round-off error
    224                         // e.g. delay=3ms, processing=4ms
    225                         if (delta - delayValue == 1)
    226                         {
    227                             // delayValue == 0 -> local clock saw no tick change but destination clock did
    228                             if (delayValue != 0)
    229                             {
    230                                 _comments.add("Info: processing time > total network time by 1 ms -> assume zero delay");
    231                                 delayValue = 0;
    232                             }
    233                         } else {
    234                            _comments.add("Warning: processing time > total network time");
    235                        }
    236                     }
    237                 }
    238                 _delay = Long.valueOf(delayValue);
    239                if (origTime > _returnTime) {
    240                    _comments.add("Error: OrigTime > DestRcvTime");
    241                }
    242
    243                _offset = Long.valueOf(((rcvTime - origTime) + (xmitTime - _returnTime)) / 2);
    244            }
    245        }
    246
    247        /**
    248         * Return list of comments (if any) during processing of NTP packet.
    249         *
    250         * @return List or null if not yet computed
    251         */
    252        public List<String> getComments()
    253        {
    254            return _comments;
    255        }
    256
    257        /**
    258         * Get round-trip network delay. If null then could not compute the delay.
    259         *
    260         * @return Long or null if delay not available.
    261         */
    262        public Long getDelay()
    263        {
    264            return _delay;
    265        }
    266
    267        /**
    268         * Get clock offset needed to adjust local clock to match remote clock. If null then could not
    269         * compute the offset.
    270         *
    271         * @return Long or null if offset not available.
    272         */
    273        public Long getOffset()
    274        {
    275            return _offset;
    276        }
    277
    278        /**
    279         * Returns NTP message packet.
    280         *
    281         * @return NTP message packet.
    282         */
    283        public NtpV3Packet getMessage()
    284        {
    285            return _message;
    286        }
    287
    288        /**
    289         * Returns time at which time message packet was received by local machine.
    290         *
    291         * @return packet return time.
    292         */
    293        public long getReturnTime()
    294        {
    295            return _returnTime;
    296        }
    297
    298    }